{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":4,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Task","Xantas","Hamilton Starlet","Eppendorf epmotion 5070"]
["Website","http://www.sias.biz/XantusJr.htm","http://www.hamiltonrobotics.com/en/hamilton-robotics/star0/","http://www.eppendorfna.com/int/index.php?l=131&sitemap=2.1&pb=7da6f876c362d435&action=products&contentid=1&catalognode=14893"]
["Liquid Pumping","Micro-annular Gear","Air Pressure","Air Pressure"]
["Water Level Sensing","capacitance","C+P","Optical confocal infrared detector:"]
["X",408,675,650]
["Y",344,465,480]
["Z",146,195,630]
["Number of Plates",12,25,4]
["Channels",1,8,8]
["Error",0.2,0.1,0.3]
["Tip Attachment",null,"Compressed O-Ring Expansion"]
["Notes","Does not define precision","Extensive Error Detection","By far the most accurate"]
[null,null,null,"Size given is total size."]
[null,null,null,"Usable area is significantly less."]
[]
[]
["All lengths in mm"]
[]
[]
[]
[]
[]
[]
["Extra Features"]
["Microplate Handling Tool","Optional","Optional - O-Ring","Optional"]
["Barcode Scanner","Optional","Optional","Standard"]
["Microplate Shaker","Optional","3rd Party Device","?"]
["Microplate Vacuum Station","Optional","Optional","?"]
["Temperature Control","Optional","3rd Party Device","Optional"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}