{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
["Item","Seller","Part #","Price ","Quantity","Total price","Purpose","Web Link"]
[]
["Air Flow Sensor","Omega","FMA-A2109",538,4,2152,"Flow in both directions for both sides of the lung","http://www.omega.com/ppt/pptsc.asp?ref=FMAA2100_2200_2300_2400&Nav=gred02"]
["Threading to Barb Adapter (1/4 NPT to 3/8\" ID) (10 pk)","Cole Parmer","EW-31702-22",15.25,2,30.5,"Connect air flow sensor to our tubing/ and to connect temp sensor in-line","http://www.coleparmer.com/catalog/product_view.asp?sku=3170222&pfx=EW"]
[]
["Fluid Flow Sensor","Omega","FTB-1411",463,4,1852,"Fluid flow in both directions of both sides of trachea","http://www.omega.com/pptst/FTB1400_Series.html"]
["Pulse to Analog Converter","Omega","DPF701-A",360,4,1440,"Convert fluid flow meter output to analog signal","http://www.omega.com/pptst/DPF700.html"]
["Threading to Barb Adapter  (1/2 NPT to 3/8\" ID)","Cole Parmer","EW-34030-97",96.5,8,772,"Connect Fluid flow sensor to our tubing","http://www.coleparmer.com/catalog/product_view.asp?sku=3403097"]
[]
["Temperature Sensor","Cole Parmer","EW-32884-00",296,4,1184,"Measure temp in both trachea and pulmonary","http://www.coleparmer.com/catalog/product_view.asp?sku=3288400&pfx=EW"]
["T-fitting (3/8\" ID) (10 pk)","Cole Parmer","EW-30703-77",32,1,32,"to be used to fit temp sensor in-line","http://www.coleparmer.com/catalog/product_view.asp?sku=3070377&pfx=EW"]
[]
["Dissolved Oxygen Sensor","Cole Parmer",null,null,4,null,"Measure DO going into both trachea and pulmonary"]
["DO Probe to Transmitter Cable","Cole Parmer",null,null,4,null,"Connect DO Probe to analog transmitter"]
["DO Transmitter","Cole Parmer",null,null,4,null,"Transmit DO Probe readings to DAQ board"]
[]
["Solenoid Valves"]
["Check Valves","Qosina",91030,2.532,40,101.28,"Check Valves ($100 is min order)","http://qosina.com/catalog/part.asp?partno=91030"]
["Panel Mount Connectors","Cole Parmer",null,null,15]
["Benchtop Tubing Cutter","Cole Parmer","06438-10",12.6,1,12.6,"Cut tubes smoothly","http://www.coleparmer.com/catalog/product_view.asp?sku=0643810"]
["Sterilizing Air Filter (10 pk)","Cole Parmer","LI-02909-55",257,1,257,"Sterilize air coming out of non sterile flow meter","http://www.coleparmer.com/catalog/product_view.asp?sku=0290955&pfx=LI"]
[]
["Pump","Cole Parmer",{"$nulls":4},"Pump media through pulmonary"]
["Pump Heads","Cole Parmer","EW-77601-10",610,2,null,"Use for pump for pulmonary side","http://www.coleparmer.com/catalog/product_view.asp?sku=7760110&pfx=EW"]
["Mounting Hardware for 2 Pump Heads","Cole Parmer","EW-77601-96",30,1,null,"Secure 2 pump heads to pump","http://www.coleparmer.com/catalog/product_view.asp?sku=7760196"]
["3/8\" ID Tubing I/P73 (50 ft)","Cole Parmer","EW-06402-73",207,1,null,"Durable tubing for above pump","http://www.coleparmer.com/catalog/product_view.asp?sku=0640273&pfx=EW"]
[]
["Elli's Compensation",{"$nulls":4},1500]
[]
[]
[{"$nulls":5},9333.380000000001]